Dome Fiber Optic Splice Closure

GJS-D007
1. Product Description
GJS-D007 dome closure is used in aerial,duct,wall-mounting,pole mounting applications, for the straight-through and branching splice of the fiber cable(Ф7-Ф42). It has heat shrinkable sealing structure with 7 entrance ports on the end (6 round ports and 1 oval port).
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2.Product Feature:

The body adopt modified plastic MPP,which is high strength and corrosion resistance,has longer lifetime and excellent sealing performance.

It has 7 cable ports in total,6 Φ20mm round cable ports,and 1 oval port which can let in and out 1pc Φ42mm cable or 2pcs Φ20mm cables,as well as for few small size cables at the same time. 
The closure can be reopened,which is maintenance friendly.It can work well in the environment of -40℃～＋65℃ and guarantee the good sealing performance.

Voltage Strength:under 15KV direct current,without breakdown or flashover phenomenon.

Insulation Resistance:≥2×104MΩ 
Tensile Force:≥800N 
Leakproofness:inflate the closure,making internal pressure to 100Kpa，then put the closure into the water over 15min,without any bubbles or pressure drop happened.

Impact Strength:can bear 16N.m.after 3 impact times,there is no crack on the body. 
Size DxH:Ф230mmx550mm

Weight:2.7Kg 
Oval port diameter:Φ42mm;round port diameter:Φ20mm

Max capacity:144cores,6pcs 24c splice tray.

Splitting:1x16/1x32 mini PLC splitters and 18pcs/36pcsSC adaptors

Assembled with valve core and grounding device.

3. Packing List:

Dome closure:1set

Hanging set:1set(optional:pole mounting,wall mounting or aerial)

Heat shrinkable tube:2~144pcs(according to the real capacity of the closure)

Hose clamp13~19: 8pcs

Shrinkable tube65/19-150: 1pc

Shrinkable tube28/6-150：6pc

Manual:1pc

Certificate of Approval:1pc

