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LAN-G1008R
Layer3 GPON OLT






Highlights
• Compact design, meets various application scenarios
Supports the deployment in diverse scenarios including low density areas, remote areas, sparsely-populated
areas and industry parks.
Supports FTTM and sharing site/rack with wireless base stations.

• Small size and lightweight, easier to delivery and install
Small size and lightweight, easy to transport and install. Supports multiple installation modes, like limited room space,basement, low-voltage room and small rack or   cabinet.


The LAN-G1008R is a pizza-box GPON OLT with
8 GPON ports that meets flexible and fast FTTx access, suiting  the scenarios such as sparse/  remote/cost-sensitive area,smart industrial
park, commercial building and  FTTM, etc.





• Carrier-class security protection, support dynamic
routing protocol RIP&OSPF, ensure the safe operation of network
Supports uplink redundancy protection including LACP STP,RSTP and MSTP, and support RIP&OSPF protocol.  Supports link
protection.

• Lower TCO
Dramatically saves on investment fees in trunk fibers, pipe
engineering, and facilities.  Effectively reduce CapEx and OpEx.


Technical Specifications

	Item
	LAN-G1008R

	Chassis
	Rack
	1U 19Inch Standard Box

	Uplink Port
	QTY
	8

	
	RJ45(GE)
	4

	
	SFP(GE)/SFP+( 10GE)
	4

	GPON Port
	QTY
	8

	
	Physical Interface
	SFP Slots

	
	Max splitting ratio
	1:128

	Management Ports
	1* 10/100/1000BASE-T out-band port, 1*CONSOLE port, 1*USB2.0, 1*Type-C USB (for console)

	Backplane Bandwidth (Gbps)
	120

	Port Forwarding Rate(Mpps)
	124.992

	

PON Port Specification
	Transmission Distance
	20KM

	
	GPON port speed
	Upstream 1.244Gbps, Downstream 2.488Gbps

	
	Wavelength
	TX 1490nm, RX 1310nm

	
	Connector
	SC/UPC

	
	Fiber Type
	9/125 μm SMF

	
	Supported PON module level
	Class B+, C, C+, C++, C+++,C++++

	Power Supply
	AC
	Working Voltage Range: 100~240V, Rated Voltage: 110V/220V

	
	DC
	Working Voltage Range: -36~-75V, Rated Voltage: -48V/-60V

	Management Mode
	EMS, WEB, SNMP, Telnet , CLI







Management Function
•  SNMP,Telnet,CLI,WEB,SSH v2;
•  Fan Group Control
•  Port Status monitoring and  configuration management
•  Online ONTconfiguration and  management
•  User management
•  Alarm management
Layer2 Switch
•  32K Mac address
•  Support 4096 VLANs
•  Support port VLAN
•  Support VLAN tag/Un-tag, VLAN transparent transmission
•  Support VLAN translation and QinQ
•  Support storm control based on port
•  Support port isolation
•  Support port rate limitation
•  Support 802.1D and 802.1W
•  Support static LACP,Dynamic LACP
•  QoS based on port, VID, TOS and MAC
address
•  Access control list
•   IEEE802.x flowcontrol
•  Port stability statistic and  monitoring
Multi cast
•   IGMP snooping
•   16K IP Multicast Groups;



DHCP
•  DHCP server,DHCP relay,DHCP snooping
•  DHCP option82

Layer 3 Route
•  ARP proxy
•   12K hardware Host Routes,12K hardware
Subnet Routes
•  Support Radius,Tacacs+
•  Support IP source guard
•  Support static route ,dynamic route RIP
v1/v2,RIPng and OSPF v2/v3;

IPv6
•  Support NDP;
•  Support IPv6 Ping,IPv6 Telnet,IPv6 routing;
•  Support ACL based on source IPv6 address,
destination IPv6 address, L4 port, protocol
type, etc;
•  Support MLD v1/v2 snooping(Multicast
Listener Discovery snooping)
GPON  Function
•  Tcont DBA
•  Gemport traffic
•   In compliant with ITU-T984.x standard
•  Up to 20KM transmission Distance
•  Support data encryption, multi-cast, port VLAN, separation, RSTP, etc
•  Support ONT auto-discovery/link
detection/remote upgrade of software


•  Support VLAN division and user
separation to avoid broadcast storm
•  Support power-off alarm function, easy
for link problem detection
•  Support broadcasting storm resistance function
•  Support port isolation between  different ports
•  Support ACL and SNMP to configure
data packet filter flexibly
•  Specialized design for system
breakdown prevention to maintain
stable system
•  Support RSTP
Dimension (L*W*H)
•  442mm*319mm*43.6mm
Weight
•  Net weight of single power: 4.14kg
•  Gross weight of single power: NAkg Power Consumption
•  40W
Working Temperature
•  -20。C ~+60。C
Storage Temperature
•   40~+70。C
Relative Humidity
•  5~95% (non-condensing)



Ordering Information:

	Product Name
	Product Description
	Power Configuration
	Accessories

	
LAN-G1008R
	

8*GPON,4*RJ45+4*SFP/SFP+
	1*AC power
2*AC power
2*DC power
1*AC power + 1* DC power
	GPON SFP C++++ module 1G SFP module
10G SFP+ module
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