PATCHCORD SC/APC-LC/APC 3.0mm Simplex G657A2 LSZH 
Specification
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Product features 
★Material for outer sheath of optical cable ：LSZH
★The structure of jumper optical cable: single core
★Connector Type ：￠3.0mm
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★Accord With ROHS 



      

SINGLE: 3.0mm     

Characteristics：

	Fiber Type

	SM G657A2

	Diameter of tight buffer fiber
	0.9mm+/-0.05

	Color of tight buffer fiber
	White

	Material of tight buffer fiber
	LSZH

	Cable diameter
	2.95+/-0.1mm

	Cable material 
	PVC

	Cable color
	White

	Strength member 
	Polyester yarn

	Tensile（N）
	Long term 50

	
	Short term 100

	crush（N/100cm）
	Long term 100

	
	Short term 200

	Bending Radius(cm)
	Dynamic 20 D

	
	Static 10 H

	Attenuation
	1310nm/1550nm≤0.34/0.21


Product type
★Types can be provided according to requirements. ：G657A2
★EXAMPLE
PATCHCORD 9/125 SC/APC-LC/APC Simplex 3.0mm G657A2 LSZH  3m

         ②        ③            ④      ⑤     ⑥     ⑦    ⑧

MODEL : PATCHCORD, 

Fiber core specification ：9/125 

Connector Type：SC/APC-LC/APC
Optical cable type：single core
Cable Diameter ：2.95±0.1mm

Optical fiber model：G657A2
Material for outer sheath of optical cable ：LSZH
LENGTH：3m，（1.98-2.05m）
Face Specification 


	Scope
	Defect description 
	Standard

	①A:
	Scratches And Nicks 
	No 

	
	Bubbles And Spots 
	No 

	
	Foreign Body 
	No 

	②B:
	Scratches And Nicks 
	No 

	
	Bubbles And Spots 
	No 

	
	Foreign Body 
	No 

	③C:
	Scratches And Nicks 
	≤2um and ≤1pcs

	
	Bubbles And Spots 
	≤2um and ≤3pcs

	
	Foreign Body 
	No

	④D:
	Scratches And Nicks 
	≤5um and ≤1pcs

	
	Bubbles And Spots 
	≤5um and ≤2pcs

	
	Foreign Body 
	No

	⑤E:
	Scratches And Nicks 
	≤5um and ≤3pcs

	
	Bubbles And Spots 
	≤5um and ≤3pcs

	
	Foreign Body 
	Allow slightly non removable


technical specifications
★Insertion Loss：IEC 61300-3-4

★Return Loss：IEC61300-3-6

★End Face Geometry：                                                   3D
UPC Radius of curvature：10～ 25mm     

APC Radius of curvature：5 ～12mm

Apex offset ：0 ～ 50um 

Optical fiber depression：+100 ～ -100 

APC Angle: 8±0.5°

★Mechanical properties ：

Durability：500 times<0.3dB

★3D APC≥70%
   UPC≥80%
Environmental technology requirements 
Transport storage environment：-40℃to+85℃

Work Environment ：-20℃to+75℃
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