Fast Connector
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product description:
1. Push-tube type fastening structure, optical fiber fastening, stable and reliable docking.
2. One-piece structure, simple structure, stable and reliable, excellent comprehensive cost.
3.Simple operation, fast construction speed, high installation success rate, long life cycle, simple and convenient post-maintenance.
Product Structure：
Measured the Structure
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Product length：
50mm ≤L≤60mm(≈54m)
Ptical Characteristics：
	Category
	Specification

	Aoolicable for
	Drop cable. Indoor cable

	Fiber mod
	Single mode or Multi mode

	Fiber type
	G.652D, G.657A2,

	Fiber cable
	3.0*2.0mm rubber-insulated optical cable 

	Fiber diameter
	0.125mm

	Force holds 2 x 3mm cable type at the beginning the fast connector
	≥ 50 N, loss ≤ 0.3 dB 

	Fiber lock
	Lock holds fiber reliability, bears hang force ≥ 1 N, attenuation changes ≤ 0.2 dB

	Working wavelength
	1310 nm, 1490 nm, 1550 nm




	Operation time
	S
	About 50(no fiber cut)

	Insertion Loss
	dB
	≤0.5

	Insertion Loss Typical value
	dB
	0.3

	Return Loss
	dB
	UPC≥50, APC≥55

	Fastening strength of naked fiber
	N
	≥3

	Tensile strength
	N
	≥45

	Reusable
	Time
	≥10 time

	Operating Temperature
	
	-40~+85

	On-line tensile strength（20N）
	dB
	ΔIL≤0.3

	Mechanical durability (500 times)
	dB
	ΔIL≤0.3

	Drop-off test (drop-off height4m, once per direction, totally 3 times)
	dB
	ΔIL≤0.3


Environmental performance requirements:
	Category
	Specification

	
	Condition
	IL Variation
	RL Variation
	Appearance

	High TEMP
	85℃, 168H
	≤0.3
	≤5
	No mechanical da mage, like deform ation, cracking and untight

	Low TEMP
	-40℃, 168H
	≤0.3
	≤5
	

	Temperature Cycle
	Cycle: 8 hours
Total: 12 cycles / 168 hours
Temperature Maintenance: 1 hour
	≤0.3
	≤5
	

	Temperature/ Humidity
	85℃, 95%RH, 168H
	≤0.3
	≤5
	

	Immersion
	25℃, 168H
	≤0.3
	≤5
	

	Salt Mis
	5% Nacl, 6.5＜PH＜ 7.5,35℃,168H
	≤0.3
	≤5
	


Mechanical Performance Requirement
	Category
	Specification

	
	Condition
	IL Variation
	RL Variation
	Appearance

	Impact
	Height: 4m; 1 drop each axis; 3 cycles
	≤0.3
	≤5
	No mechanical da mage, like deforma tion, cracking and untight

	Vibration
	Frequency: 10 ～ 50HZ;
Sweep: 45 times / min;
amplitude: 0.75mm;
Duration:30min each axial
	≤0.3
	≤5
	

	Torsional
	Pull：15N; The distance between Loading location and fast connector: L = 22-28cm; Rate：10times / min. Times:
	≤0.3
	≤5
	




	Tensile
	Pull：50N; The distance between Loading lo cation and fast connector: L = 3M; Duration:1min
	≤0.3
	≤5
	


Product Packaging Information：
Blister Box Packing

Adapter (supports strip and cut fiber)：
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