
Product Specification

10Gbps 10KM SFP+ Transceiver
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Diagram of Host Board Connector Block Pin Numbers and Names



SFP+10G-13-20
Product Features 

Up to 10Gbps data links

20km with 9/125µm SMF
1310nm DFB laser
Duplex LC Connector

Hot-pluggable SFP+ footprint             

Single 3. 3V power supply              Applications
Operating temperature: 0℃ to 70℃      √  10GBase-LR/LW 10G Ethernet 
RoHS                              √  1200-SM-LL-L 10G FC
Digital Diagnostic Monitor compatible
Power Consumption < 0.8W
1. Product Description 

The SFP+10G-13-20 is a 10Gbps enhanced small form factor pluggable SFP+ transceiver compatible with 10GBASE-LR/LW and 10G Fiber Channel 1200-SM-LL-L. It is suitable for single-mode fiber (SMF) communications in 10Gbps Ethernet and 10G Fiber Channel. 

2. Regulatory Compliance

Transceivers are Class 1 Laser Products comply with FDA regulations. Meet Class 1 eye safety requirements of EN 60825 and the electrical safety requirements of EN 60950.

3. Absolute Maximum Ratings

	Parameter 
	Symbol 
	Min. 
	Max. 
	Unit 

	Supply Voltage 
	VCC 
	-0.5 
	4
	V 

	Storage Temperature 
	TS 
	-40 
	85 
	°C 

	Operating Case Temperature 
	TC
	0 
	70
	°C 


4. Recommended Operating Conditions
	Parameter
	Symbol
	Min. 
	Typical 
	Max. 
	Unit 

	Operating Case Temperature
	TC 
	0
	
	70
	°C

	Power Supply Voltage 
	VCC 
	3.15
	3.3 
	3.45 
	V 

	Power Supply Current 
	ICC 
	
	
	200 
	mA 

	Data Rate 
	
	
	10
	
	GBps 

	Max Link Length on 9/125µm SMF 
	Lmax
	
	10
	
	km


5. Optical Characteristics
	Parameter
	Symbol 
	Min. 
	Typical 
	Max. 
	Unit 

	Transmitter

	Centre Wavelength 
	λc 
	1260 
	1310 
	1360 
	nm 

	Spectral Width (-20dB) 
	σ
	
	
	1
	nm 

	Average Output Power 
	Pout 
	-5 
	
	0
	dBm 

	Extinction Ratio 
	ER 
	3.5 
	
	
	dB 

	Average Launch Power of Off Transmitter 
	Poff
	
	
	-30
	dBm 

	Receiver 

	Centre Wavelength 
	λc 
	1200 
	1310
	1600 
	nm 

	Receiver Sensitivity 
	PIN 
	
	
	-14
	dBm 

	Receiver Overload
	Pmax
	0.5
	
	
	dBm

	LOS De-Assert 
	LOSD 
	
	
	-19
	dBm 

	LOS Assert 
	LOSA 
	-24 
	
	
	dBm 

	LOS Hysteresis
	
	0.5
	
	4.5
	dB


6. Electrical Characteristics
	Parameter
	Symbol 
	Min. 
	Typical 
	Max. 
	Unit 

	Transmitter

	Input Differential Impedance
	Zin 
	90 
	100
	110 
	Ω 

	Data Input Swing Differential 
	Vin 
	250 
	
	1200 
	mV 

	Tx-Dis Disable 
	Vd 
	2.0 
	
	Vcc
	V 

	Tx-Dis Enable 
	Ven 
	0 
	
	0.8
	V 

	Receiver 

	Data Output Swing Differential 
	Vout 
	250 
	
	800 
	mV 

	Rx-Los Fault
	Vlf
	2.0
	
	VccHOST 
	V 

	Rx-Los Normal
	Vln
	0
	
	0+0.8
	V

	Output rise and fall time
	Tr, Tf
	30
	
	
	ps


7. Pin Descriptions
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	Pin 
	Symbol 
	Description 
	Ref. 

	1 
	VEET 
	Transmitter Ground  (Common with Receiver Ground) 
	7.1 

	2 
	TFAULT 
	Transmitter Fault.  
	

	3 
	TDIS 
	Transmitter Disable. Laser output disabled on high or open. 
	7.2 

	4 
	MOD_DEF(2) 
	Module Definition 2. Data line for Serial ID. 
	7.3 

	5 
	MOD_DEF(1) 
	Module Definition 1. Clock line for Serial ID. 
	7.3 

	6 
	MOD_DEF(0) 
	Module Definition 0. Grounded within the module. 
	7.3 

	7 
	RS0
	Rate Select0, optionally controls SFP+ module receiver. When high input signaling rate>4.25 GBd and when low input signaling rate<4.25GBd
	

	8 
	LOS 
	Loss of Signal indication.  Logic 0 indicates normal operation. 
	7.4

	9 
	RS1
	Rate Select1, optionally controls SFP+ module receiver. When high input signaling rate>4.25 GBd and when low input signaling rate<4.25GBd
	

	10 
	VEER 
	Receiver Ground  (Common with Transmitter Ground) 
	7.1 

	11 
	VEER 
	Receiver Ground  (Common with Transmitter Ground) 
	7.1 

	12 
	RD-
	Receiver Inverted DATA out.  AC Coupled. 
	

	13 
	RD+ 
	Receiver Non-inverted DATA out.  AC Coupled. 
	

	14 
	VEER 
	Receiver Ground  (Common with Transmitter Ground) 
	7.1 

	15 
	VCCR 
	Receiver Power Supply 
	

	16 
	VCCT 
	Transmitter Power Supply 
	

	17 
	VEET 
	Transmitter Ground  (Common with Receiver Ground) 
	7.1 

	18 
	TD+ 
	Transmitter Non-Inverted DATA in.  AC Coupled. 
	

	19 
	TD-
	Transmitter Inverted DATA in.  AC Coupled. 
	

	20 
	VEET 
	Transmitter Ground  (Common with Receiver Ground) 
	7.1 


Notes: 

7.1 Circuit ground is internally isolated from chassis ground. 

7.2 Laser output disabled on TDIS >2.0V or open, enabled on TDIS <0.8V. 

7.3 Should be pulled up with 4.7k - 10kohms on host board to a voltage between 2.0V and 3.6V. MOD_DEF(0) pulls line low to indicate module is plugged in. 

7.4 LOS is open collector output.  Should be pulled up with 4.7k -10kohms on host board to a voltage between 2.0V and 3.6V. Logic 0 indicates normal operation; logic 1 indicates loss of signal. 

8. EEPROM & DDM THRESHOLD 

8.1 EEPROM

2 wire address 1010000X (A0h)

	0~95

Serial ID Defined by SFP MSA (96 bytes)

	96~127

Vendor Speific (32 bytes)

	128~255

Reserved (128 bytes)


8.1 DDM THRESHOLD

	
	Low Alarm
	Low Warn
	High Warn
	High Alarm

	Temperature
	-5℃
	0℃
	70℃
	75℃

	Voltage
	3V
	3.1V
	3.6V
	3.7V

	Tx Bias
	15mA
	20mA
	75mA
	85mA

	Tx Power
	-8.5dBm
	-7.5dBm
	0dBm
	0.5dBm

	Rx Power
	-18.5dBm
	-16dBm
	0.5dBm
	1.5dBm


9. Mechanical Specifications
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10. LABEL

offers label OEM design and print. Label barcode supports code 128 and 2D barcode 
SIZE:  30mm*9mm   
Ordering Information
	Part No.
	Data Rate
	DDM
	Wave
	Fiber Type
	Dist.
	Temp.
	Optical Interface

	SFP+10G-13-20 
	10Gbps
	yes
	1310nm
	SMF
	20km
	0~70℃
	LC
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