Packing Details for Reference (or Meet Customized Standard)


10 Ports Non-open Pre-connectorized Fiber Access
FastConnect Terminal Box


Product Overview


[bookmark: _GoBack]Fiber access terminal box (FAT) also named as optical termination box (OTB), is a compact fiber management box used for FTTH application. Fiber termination box (FTB) is widely used in FTTx cabling for both fiber cabling and cable management.
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Application

1) FTTH;
2) FTTA;
3) Trunk Cable Connecting.


Feature
1) High compatibility support harden adapter of OptiTap, Slim and FastConnect;
2) Strong enough: working under 1000N pulling force long term;
3) Installation on Wall/Pole/Aerial mounted, underground;;
4) Available with PLC fiber divide;
5) Decreased angle surface and height make sure no connector interfering when operating;
6) Cost effective: save 40% operating time and less manpower.

Technical Parameter

	Model
	Total Value (dB)
	1x2 FBT High Power (dB)
	1x2 FBT + 1x8 PLC (dB)

	90/10
	≤21.54
	≤ 0.73
	≤ (11.04+10.5)

	85/15
	≤ 20.78
	≤ 1.13
	≤ (10.28+10.5)

	80/20
	≤ 18.25
	≤ 1.25
	≤ (7.75+10.5)

	70/30
	≤ 16.51
	≤ 2.22
	≤ (6.01+10.5)

	60/40
	≤ 15.32
	≤ 2.73
	≤ (4.82+10.5)

	1:8
	≤ 10.50
	≤ N/A
	≤ 10.5



Specification Details

	Dimension (L x W x H)
	198 x 160 x 70mm

	Waterproof Level
	IP68

	Port Type Solution
	10pcs of Harden FastConnect Adapters

	Color
	Black

	Material
	PC + ABS

	Max Capacity
	10 Ports

	UV resistance
	ISO 4892-3

	Fire protection rating
	UL94-V0

	Number of PLC (Solution)
	1x2 FBT Uneven PLC + 1x8 PLC

	Warranty Life Time (Non-artificial damage)
	5 Years



Mechanical Parameter

	Atmospheric Pressure
	70KPa~106Kpa

	Lid opening angle for operating
	No, 100% sealed off (Ultrasonic crimping)

	Tensile Resistance
	＞1000N

	Crush Resistance
	＞2000N/10cm2 Pressure, time 1min

	Insulation resistance
	＞2×104MΩ

	Compressive Strength
	15KV(DC)/1min no breakdown and no arcing.

	Relative Humidity
	≤93％ (+40℃)







	Storage Temperature
	-40℃ ～ +85℃

	Operating Temperature
	-40℃ ～ +60℃

	Installation Temperature
	-40℃ ～ +60℃



Application Scheme
➋ 3 PCS Uneven Box
➊ Fiber Cable
➌ End Box
➋ Drop Flat Cable
1x9
1 FO
1x9
1 FO
1x9
1 FO
1x8
50m
50m
50m
1 FO
➊ Hub Box
1 FO
1 FO
CO
MDU single fiber solution
Indoor Duct
Outdoor multi-fiber solutions
Ground
Outdoor single fiber solution
Ground / Duct




PLC Splitter Diagram

Drawing of PLC Splitter: 1 x 9 Solution



Port 135mm
1:8 PLC Splitter
15cm
1: 2 FBT, 60/40, 70/30, 80/20
85/15, 90/10 Optional	INPUT
S/N: XXXXXXXXX
50cm
50cm

SC/APC Connector (Green Color)
900um Loose Tube 8 Colors
SC/APC Connector (Green Color)

Port 2
Port 3Side B

Port 4Side A

Port 5
Port 6
Port 7
Port 8
Environmental Characteristics
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Including Accessories

	Item Description
	Picture
	Qty

	

L40mm Screw
	
[image: ]
	
4

	Ø15mm*6mm
Hex Socket Head Cap Screw
	
[image: ]
	4

	Ø20mm*6mm
Hex Socket Head Cap Screw
	
[image: ]
	4

	Ø8mm*3.5mm
Hex Nuts
	
[image: ]
	4

	Ø8mm*40mm
Drilling drywall anchors
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4

	Ø9mm Metal Lock Washer
	
[image: ]
	4

	

Ø260mm Stainless Steel Hose Ring
	
[image: ]
	
2

	Ø3mm*12cm
L Handle Allen Wrench Kit
	
[image: ]
	
1

	Wing Nuts 304 Stainless
	
[image: ]
	4

	

Cable Storage Kits
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2

	

Aerial-mounted Kit
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2


Products Drawing (Unit: mm)




Product Inner Box Packing

	
[image: ]
	Size (cm)
	25cm*25cm*13cm

	
	QTY (pcs/box)
	1

	
	

Net Weight (kg/pcs)
	

0.61



Accessories Inner Box Packing

	
[image: ]
	Size (cm)
	25*25**15cm

	
	Set
	8pcs/set

	
	G.W (kg/box)
	0.6



Master Carton for Product

	
[image: ]
	Size (cm)
	63cm*50cm*48cm

	
	QTY (pcs/box)
	12

	
	Net Weight (kg/Carton)
	7.2



Master Carton for Accessories

	
[image: ]
	Size (cm)
	63cm*50cm*48cm

	
	QTY (Sets/box)
	12

	
	Net Weight (kg/Carton)
	7.5
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